# Austria, all DVB-T transmitters run by ORS
# Created from
# http://www.ors.at/fileadmin/user_upload/downloads/DVB-T_Kanalbezeichnungen_und_Mittenfrequenzen.pdf
[CHANNEL]
	DELIVERY_SYSTEM = DVBT
	FREQUENCY = 474000000
	BANDWIDTH_HZ = 8000000
	CODE_RATE_HP = 3/4
	CODE_RATE_LP = NONE
	MODULATION = QAM/16
	TRANSMISSION_MODE = 8K
	GUARD_INTERVAL = 1/4
	HIERARCHY = NONE
	INVERSION = AUTO

[CHANNEL]
	DELIVERY_SYSTEM = DVBT
	FREQUENCY = 482000000
	BANDWIDTH_HZ = 8000000
	CODE_RATE_HP = 3/4
	CODE_RATE_LP = NONE
	MODULATION = QAM/16
	TRANSMISSION_MODE = 8K
	GUARD_INTERVAL = 1/4
	HIERARCHY = NONE
	INVERSION = AUTO

[CHANNEL]
	DELIVERY_SYSTEM = DVBT
	FREQUENCY = 490000000
	BANDWIDTH_HZ = 8000000
	CODE_RATE_HP = 3/4
	CODE_RATE_LP = NONE
	MODULATION = QAM/16
	TRANSMISSION_MODE = 8K
	GUARD_INTERVAL = 1/4
	HIERARCHY = NONE
	INVERSION = AUTO

[CHANNEL]
	DELIVERY_SYSTEM = DVBT
	FREQUENCY = 498000000
	BANDWIDTH_HZ = 8000000
	CODE_RATE_HP = 3/4
	CODE_RATE_LP = NONE
	MODULATION = QAM/16
	TRANSMISSION_MODE = 8K
	GUARD_INTERVAL = 1/4
	HIERARCHY = NONE
	INVERSION = AUTO

[CHANNEL]
	DELIVERY_SYSTEM = DVBT
	FREQUENCY = 506000000
	BANDWIDTH_HZ = 8000000
	CODE_RATE_HP = 3/4
	CODE_RATE_LP = NONE
	MODULATION = QAM/16
	TRANSMISSION_MODE = 8K
	GUARD_INTERVAL = 1/4
	HIERARCHY = NONE
	INVERSION = AUTO

[CHANNEL]
	DELIVERY_SYSTEM = DVBT
	FREQUENCY = 514000000
	BANDWIDTH_HZ = 8000000
	CODE_RATE_HP = 3/4
	CODE_RATE_LP = NONE
	MODULATION = QAM/16
	TRANSMISSION_MODE = 8K
	GUARD_INTERVAL = 1/4
	HIERARCHY = NONE
	INVERSION = AUTO

[CHANNEL]
	DELIVERY_SYSTEM = DVBT
	FREQUENCY = 522000000
	BANDWIDTH_HZ = 8000000
	CODE_RATE_HP = 3/4
	CODE_RATE_LP = NONE
	MODULATION = QAM/16
	TRANSMISSION_MODE = 8K
	GUARD_INTERVAL = 1/4
	HIERARCHY = NONE
	INVERSION = AUTO

[CHANNEL]
	DELIVERY_SYSTEM = DVBT
	FREQUENCY = 530000000
	BANDWIDTH_HZ = 8000000
	CODE_RATE_HP = 3/4
	CODE_RATE_LP = NONE
	MODULATION = QAM/16
	TRANSMISSION_MODE = 8K
	GUARD_INTERVAL = 1/4
	HIERARCHY = NONE
	INVERSION = AUTO

[CHANNEL]
	DELIVERY_SYSTEM = DVBT
	FREQUENCY = 538000000
	BANDWIDTH_HZ = 8000000
	CODE_RATE_HP = 3/4
	CODE_RATE_LP = NONE
	MODULATION = QAM/16
	TRANSMISSION_MODE = 8K
	GUARD_INTERVAL = 1/4
	HIERARCHY = NONE
	INVERSION = AUTO

[CHANNEL]
	DELIVERY_SYSTEM = DVBT
	FREQUENCY = 546000000
	BANDWIDTH_HZ = 8000000
	CODE_RATE_HP = 3/4
	CODE_RATE_LP = NONE
	MODULATION = QAM/16
	TRANSMISSION_MODE = 8K
	GUARD_INTERVAL = 1/4
	HIERARCHY = NONE
	INVERSION = AUTO

[CHANNEL]
	DELIVERY_SYSTEM = DVBT
	FREQUENCY = 554000000
	BANDWIDTH_HZ = 8000000
	CODE_RATE_HP = 3/4
	CODE_RATE_LP = NONE
	MODULATION = QAM/16
	TRANSMISSION_MODE = 8K
	GUARD_INTERVAL = 1/4
	HIERARCHY = NONE
	INVERSION = AUTO

[CHANNEL]
	DELIVERY_SYSTEM = DVBT
	FREQUENCY = 562000000
	BANDWIDTH_HZ = 8000000
	CODE_RATE_HP = 3/4
	CODE_RATE_LP = NONE
	MODULATION = QAM/16
	TRANSMISSION_MODE = 8K
	GUARD_INTERVAL = 1/4
	HIERARCHY = NONE
	INVERSION = AUTO

[CHANNEL]
	DELIVERY_SYSTEM = DVBT
	FREQUENCY = 570000000
	BANDWIDTH_HZ = 8000000
	CODE_RATE_HP = 3/4
	CODE_RATE_LP = NONE
	MODULATION = QAM/16
	TRANSMISSION_MODE = 8K
	GUARD_INTERVAL = 1/4
	HIERARCHY = NONE
	INVERSION = AUTO

[CHANNEL]
	DELIVERY_SYSTEM = DVBT
	FREQUENCY = 578000000
	BANDWIDTH_HZ = 8000000
	CODE_RATE_HP = 3/4
	CODE_RATE_LP = NONE
	MODULATION = QAM/16
	TRANSMISSION_MODE = 8K
	GUARD_INTERVAL = 1/4
	HIERARCHY = NONE
	INVERSION = AUTO

[CHANNEL]
	DELIVERY_SYSTEM = DVBT
	FREQUENCY = 578000000
	BANDWIDTH_HZ = 8000000
	CODE_RATE_HP = 3/4
	CODE_RATE_LP = NONE
	MODULATION = QAM/16
	TRANSMISSION_MODE = 8K
	GUARD_INTERVAL = 1/8
	HIERARCHY = NONE
	INVERSION = AUTO

[CHANNEL]
	DELIVERY_SYSTEM = DVBT
	FREQUENCY = 586000000
	BANDWIDTH_HZ = 8000000
	CODE_RATE_HP = 3/4
	CODE_RATE_LP = NONE
	MODULATION = QAM/16
	TRANSMISSION_MODE = 8K
	GUARD_INTERVAL = 1/4
	HIERARCHY = NONE
	INVERSION = AUTO

[CHANNEL]
	DELIVERY_SYSTEM = DVBT
	FREQUENCY = 594000000
	BANDWIDTH_HZ = 8000000
	CODE_RATE_HP = 3/4
	CODE_RATE_LP = NONE
	MODULATION = QAM/16
	TRANSMISSION_MODE = 8K
	GUARD_INTERVAL = 1/4
	HIERARCHY = NONE
	INVERSION = AUTO

[CHANNEL]
	DELIVERY_SYSTEM = DVBT
	FREQUENCY = 602000000
	BANDWIDTH_HZ = 8000000
	CODE_RATE_HP = 3/4
	CODE_RATE_LP = NONE
	MODULATION = QAM/16
	TRANSMISSION_MODE = 8K
	GUARD_INTERVAL = 1/4
	HIERARCHY = NONE
	INVERSION = AUTO

[CHANNEL]
	DELIVERY_SYSTEM = DVBT
	FREQUENCY = 610000000
	BANDWIDTH_HZ = 8000000
	CODE_RATE_HP = 3/4
	CODE_RATE_LP = NONE
	MODULATION = QAM/16
	TRANSMISSION_MODE = 8K
	GUARD_INTERVAL = 1/4
	HIERARCHY = NONE
	INVERSION = AUTO

[CHANNEL]
	DELIVERY_SYSTEM = DVBT
	FREQUENCY = 618000000
	BANDWIDTH_HZ = 8000000
	CODE_RATE_HP = 3/4
	CODE_RATE_LP = NONE
	MODULATION = QAM/16
	TRANSMISSION_MODE = 8K
	GUARD_INTERVAL = 1/4
	HIERARCHY = NONE
	INVERSION = AUTO

[CHANNEL]
	DELIVERY_SYSTEM = DVBT
	FREQUENCY = 626000000
	BANDWIDTH_HZ = 8000000
	CODE_RATE_HP = 3/4
	CODE_RATE_LP = NONE
	MODULATION = QAM/16
	TRANSMISSION_MODE = 8K
	GUARD_INTERVAL = 1/4
	HIERARCHY = NONE
	INVERSION = AUTO

[CHANNEL]
	DELIVERY_SYSTEM = DVBT
	FREQUENCY = 634000000
	BANDWIDTH_HZ = 8000000
	CODE_RATE_HP = 3/4
	CODE_RATE_LP = NONE
	MODULATION = QAM/16
	TRANSMISSION_MODE = 8K
	GUARD_INTERVAL = 1/4
	HIERARCHY = NONE
	INVERSION = AUTO

[CHANNEL]
	DELIVERY_SYSTEM = DVBT
	FREQUENCY = 642000000
	BANDWIDTH_HZ = 8000000
	CODE_RATE_HP = 3/4
	CODE_RATE_LP = NONE
	MODULATION = QAM/16
	TRANSMISSION_MODE = 8K
	GUARD_INTERVAL = 1/4
	HIERARCHY = NONE
	INVERSION = AUTO

[CHANNEL]
	DELIVERY_SYSTEM = DVBT
	FREQUENCY = 650000000
	BANDWIDTH_HZ = 8000000
	CODE_RATE_HP = 3/4
	CODE_RATE_LP = NONE
	MODULATION = QAM/16
	TRANSMISSION_MODE = 8K
	GUARD_INTERVAL = 1/4
	HIERARCHY = NONE
	INVERSION = AUTO

[CHANNEL]
	DELIVERY_SYSTEM = DVBT
	FREQUENCY = 658000000
	BANDWIDTH_HZ = 8000000
	CODE_RATE_HP = 3/4
	CODE_RATE_LP = NONE
	MODULATION = QAM/16
	TRANSMISSION_MODE = 8K
	GUARD_INTERVAL = 1/4
	HIERARCHY = NONE
	INVERSION = AUTO

[CHANNEL]
	DELIVERY_SYSTEM = DVBT
	FREQUENCY = 666000000
	BANDWIDTH_HZ = 8000000
	CODE_RATE_HP = 3/4
	CODE_RATE_LP = NONE
	MODULATION = QAM/16
	TRANSMISSION_MODE = 8K
	GUARD_INTERVAL = 1/4
	HIERARCHY = NONE
	INVERSION = AUTO

[CHANNEL]
	DELIVERY_SYSTEM = DVBT
	FREQUENCY = 674000000
	BANDWIDTH_HZ = 8000000
	CODE_RATE_HP = 3/4
	CODE_RATE_LP = NONE
	MODULATION = QAM/16
	TRANSMISSION_MODE = 8K
	GUARD_INTERVAL = 1/4
	HIERARCHY = NONE
	INVERSION = AUTO

[CHANNEL]
	DELIVERY_SYSTEM = DVBT
	FREQUENCY = 682000000
	BANDWIDTH_HZ = 8000000
	CODE_RATE_HP = 3/4
	CODE_RATE_LP = NONE
	MODULATION = QAM/16
	TRANSMISSION_MODE = 8K
	GUARD_INTERVAL = 1/4
	HIERARCHY = NONE
	INVERSION = AUTO

[CHANNEL]
	DELIVERY_SYSTEM = DVBT
	FREQUENCY = 690000000
	BANDWIDTH_HZ = 8000000
	CODE_RATE_HP = 3/4
	CODE_RATE_LP = NONE
	MODULATION = QAM/16
	TRANSMISSION_MODE = 8K
	GUARD_INTERVAL = 1/4
	HIERARCHY = NONE
	INVERSION = AUTO

[CHANNEL]
	DELIVERY_SYSTEM = DVBT
	FREQUENCY = 698000000
	BANDWIDTH_HZ = 8000000
	CODE_RATE_HP = 3/4
	CODE_RATE_LP = NONE
	MODULATION = QAM/16
	TRANSMISSION_MODE = 8K
	GUARD_INTERVAL = 1/4
	HIERARCHY = NONE
	INVERSION = AUTO

[CHANNEL]
	DELIVERY_SYSTEM = DVBT
	FREQUENCY = 706000000
	BANDWIDTH_HZ = 8000000
	CODE_RATE_HP = 3/4
	CODE_RATE_LP = NONE
	MODULATION = QAM/16
	TRANSMISSION_MODE = 8K
	GUARD_INTERVAL = 1/4
	HIERARCHY = NONE
	INVERSION = AUTO

[CHANNEL]
	DELIVERY_SYSTEM = DVBT
	FREQUENCY = 714000000
	BANDWIDTH_HZ = 8000000
	CODE_RATE_HP = 3/4
	CODE_RATE_LP = NONE
	MODULATION = QAM/16
	TRANSMISSION_MODE = 8K
	GUARD_INTERVAL = 1/4
	HIERARCHY = NONE
	INVERSION = AUTO

[CHANNEL]
	DELIVERY_SYSTEM = DVBT
	FREQUENCY = 722000000
	BANDWIDTH_HZ = 8000000
	CODE_RATE_HP = 3/4
	CODE_RATE_LP = NONE
	MODULATION = QAM/16
	TRANSMISSION_MODE = 8K
	GUARD_INTERVAL = 1/4
	HIERARCHY = NONE
	INVERSION = AUTO

[CHANNEL]
	DELIVERY_SYSTEM = DVBT
	FREQUENCY = 730000000
	BANDWIDTH_HZ = 8000000
	CODE_RATE_HP = 3/4
	CODE_RATE_LP = NONE
	MODULATION = QAM/16
	TRANSMISSION_MODE = 8K
	GUARD_INTERVAL = 1/4
	HIERARCHY = NONE
	INVERSION = AUTO

[CHANNEL]
	DELIVERY_SYSTEM = DVBT
	FREQUENCY = 738000000
	BANDWIDTH_HZ = 8000000
	CODE_RATE_HP = 3/4
	CODE_RATE_LP = NONE
	MODULATION = QAM/16
	TRANSMISSION_MODE = 8K
	GUARD_INTERVAL = 1/4
	HIERARCHY = NONE
	INVERSION = AUTO

[CHANNEL]
	DELIVERY_SYSTEM = DVBT
	FREQUENCY = 746000000
	BANDWIDTH_HZ = 8000000
	CODE_RATE_HP = 3/4
	CODE_RATE_LP = NONE
	MODULATION = QAM/16
	TRANSMISSION_MODE = 8K
	GUARD_INTERVAL = 1/4
	HIERARCHY = NONE
	INVERSION = AUTO

[CHANNEL]
	DELIVERY_SYSTEM = DVBT
	FREQUENCY = 754000000
	BANDWIDTH_HZ = 8000000
	CODE_RATE_HP = 3/4
	CODE_RATE_LP = NONE
	MODULATION = QAM/16
	TRANSMISSION_MODE = 8K
	GUARD_INTERVAL = 1/4
	HIERARCHY = NONE
	INVERSION = AUTO

[CHANNEL]
	DELIVERY_SYSTEM = DVBT
	FREQUENCY = 762000000
	BANDWIDTH_HZ = 8000000
	CODE_RATE_HP = 3/4
	CODE_RATE_LP = NONE
	MODULATION = QAM/16
	TRANSMISSION_MODE = 8K
	GUARD_INTERVAL = 1/4
	HIERARCHY = NONE
	INVERSION = AUTO

[CHANNEL]
	DELIVERY_SYSTEM = DVBT
	FREQUENCY = 770000000
	BANDWIDTH_HZ = 8000000
	CODE_RATE_HP = 3/4
	CODE_RATE_LP = NONE
	MODULATION = QAM/16
	TRANSMISSION_MODE = 8K
	GUARD_INTERVAL = 1/4
	HIERARCHY = NONE
	INVERSION = AUTO

[CHANNEL]
	DELIVERY_SYSTEM = DVBT
	FREQUENCY = 778000000
	BANDWIDTH_HZ = 8000000
	CODE_RATE_HP = 3/4
	CODE_RATE_LP = NONE
	MODULATION = QAM/16
	TRANSMISSION_MODE = 8K
	GUARD_INTERVAL = 1/4
	HIERARCHY = NONE
	INVERSION = AUTO

[CHANNEL]
	DELIVERY_SYSTEM = DVBT
	FREQUENCY = 786000000
	BANDWIDTH_HZ = 8000000
	CODE_RATE_HP = 3/4
	CODE_RATE_LP = NONE
	MODULATION = QAM/16
	TRANSMISSION_MODE = 8K
	GUARD_INTERVAL = 1/4
	HIERARCHY = NONE
	INVERSION = AUTO

[CHANNEL]
	DELIVERY_SYSTEM = DVBT
	FREQUENCY = 794000000
	BANDWIDTH_HZ = 8000000
	CODE_RATE_HP = 3/4
	CODE_RATE_LP = NONE
	MODULATION = QAM/16
	TRANSMISSION_MODE = 8K
	GUARD_INTERVAL = 1/4
	HIERARCHY = NONE
	INVERSION = AUTO

[CHANNEL]
	DELIVERY_SYSTEM = DVBT
	FREQUENCY = 802000000
	BANDWIDTH_HZ = 8000000
	CODE_RATE_HP = 3/4
	CODE_RATE_LP = NONE
	MODULATION = QAM/16
	TRANSMISSION_MODE = 8K
	GUARD_INTERVAL = 1/4
	HIERARCHY = NONE
	INVERSION = AUTO

[CHANNEL]
	DELIVERY_SYSTEM = DVBT
	FREQUENCY = 810000000
	BANDWIDTH_HZ = 8000000
	CODE_RATE_HP = 3/4
	CODE_RATE_LP = NONE
	MODULATION = QAM/16
	TRANSMISSION_MODE = 8K
	GUARD_INTERVAL = 1/4
	HIERARCHY = NONE
	INVERSION = AUTO

[CHANNEL]
	DELIVERY_SYSTEM = DVBT
	FREQUENCY = 826000000
	BANDWIDTH_HZ = 8000000
	CODE_RATE_HP = 3/4
	CODE_RATE_LP = NONE
	MODULATION = QAM/16
	TRANSMISSION_MODE = 8K
	GUARD_INTERVAL = 1/4
	HIERARCHY = NONE
	INVERSION = AUTO

[CHANNEL]
	DELIVERY_SYSTEM = DVBT
	FREQUENCY = 834000000
	BANDWIDTH_HZ = 8000000
	CODE_RATE_HP = 3/4
	CODE_RATE_LP = NONE
	MODULATION = QAM/16
	TRANSMISSION_MODE = 8K
	GUARD_INTERVAL = 1/4
	HIERARCHY = NONE
	INVERSION = AUTO

[CHANNEL]
	DELIVERY_SYSTEM = DVBT
	FREQUENCY = 842000000
	BANDWIDTH_HZ = 8000000
	CODE_RATE_HP = 3/4
	CODE_RATE_LP = NONE
	MODULATION = QAM/16
	TRANSMISSION_MODE = 8K
	GUARD_INTERVAL = 1/4
	HIERARCHY = NONE
	INVERSION = AUTO

[CHANNEL]
	DELIVERY_SYSTEM = DVBT
	FREQUENCY = 850000000
	BANDWIDTH_HZ = 8000000
	CODE_RATE_HP = 3/4
	CODE_RATE_LP = NONE
	MODULATION = QAM/16
	TRANSMISSION_MODE = 8K
	GUARD_INTERVAL = 1/4
	HIERARCHY = NONE
	INVERSION = AUTO

[CHANNEL]
	DELIVERY_SYSTEM = DVBT
	FREQUENCY = 858000000
	BANDWIDTH_HZ = 8000000
	CODE_RATE_HP = 3/4
	CODE_RATE_LP = NONE
	MODULATION = QAM/16
	TRANSMISSION_MODE = 8K
	GUARD_INTERVAL = 1/4
	HIERARCHY = NONE
	INVERSION = AUTO

