# 2014-03-08 Olli Salonen <olli.salonen@iki.fi>
# generated from http://www.dna.fi/tuki-antenniverkon-nakyvyysalueet
[CHANNEL]
	DELIVERY_SYSTEM = DVBT2
	FREQUENCY = 219500000
	BANDWIDTH_HZ = 7000000
	CODE_RATE_HP = AUTO
	CODE_RATE_LP = AUTO
	MODULATION = QAM/AUTO
	TRANSMISSION_MODE = 32K
	GUARD_INTERVAL = 19/256
	HIERARCHY = AUTO
	INVERSION = AUTO

[CHANNEL]
	DELIVERY_SYSTEM = DVBT2
	FREQUENCY = 226500000
	BANDWIDTH_HZ = 7000000
	CODE_RATE_HP = AUTO
	CODE_RATE_LP = AUTO
	MODULATION = QAM/AUTO
	TRANSMISSION_MODE = 32K
	GUARD_INTERVAL = 19/256
	HIERARCHY = AUTO
	INVERSION = AUTO

[CHANNEL]
	DELIVERY_SYSTEM = DVBT2
	FREQUENCY = 212500000
	BANDWIDTH_HZ = 7000000
	CODE_RATE_HP = AUTO
	CODE_RATE_LP = AUTO
	MODULATION = QAM/AUTO
	TRANSMISSION_MODE = 32K
	GUARD_INTERVAL = 19/256
	HIERARCHY = AUTO
	INVERSION = AUTO

