# Australia / QLD / Fraser Coast - Bundaberg / Mt Goonaneman
# ABC VHF9A
[CHANNEL]
	DELIVERY_SYSTEM = DVBT
	FREQUENCY = 205625000
	BANDWIDTH_HZ = 7000000
	CODE_RATE_HP = 3/4
	CODE_RATE_LP = NONE
	MODULATION = QAM/64
	TRANSMISSION_MODE = 8K
	GUARD_INTERVAL = 1/16
	HIERARCHY = NONE
	INVERSION = AUTO

# SBS UHF28
[CHANNEL]
	DELIVERY_SYSTEM = DVBT
	FREQUENCY = 529500000
	BANDWIDTH_HZ = 7000000
	CODE_RATE_HP = 2/3
	CODE_RATE_LP = NONE
	MODULATION = QAM/64
	TRANSMISSION_MODE = 8K
	GUARD_INTERVAL = 1/8
	HIERARCHY = NONE
	INVERSION = AUTO

# Seven VHF7
[CHANNEL]
	DELIVERY_SYSTEM = DVBT
	FREQUENCY = 184625000
	BANDWIDTH_HZ = 7000000
	CODE_RATE_HP = 2/3
	CODE_RATE_LP = NONE
	MODULATION = QAM/64
	TRANSMISSION_MODE = 8K
	GUARD_INTERVAL = 1/16
	HIERARCHY = NONE
	INVERSION = AUTO

# WIN Wide Bay VHF10
[CHANNEL]
	DELIVERY_SYSTEM = DVBT
	FREQUENCY = 212500000
	BANDWIDTH_HZ = 7000000
	CODE_RATE_HP = 3/4
	CODE_RATE_LP = NONE
	MODULATION = QAM/64
	TRANSMISSION_MODE = 8K
	GUARD_INTERVAL = 1/16
	HIERARCHY = NONE
	INVERSION = AUTO

# Southern Cross Ten VHF9
[CHANNEL]
	DELIVERY_SYSTEM = DVBT
	FREQUENCY = 198525000
	BANDWIDTH_HZ = 7000000
	CODE_RATE_HP = 3/4
	CODE_RATE_LP = NONE
	MODULATION = QAM/64
	TRANSMISSION_MODE = 8K
	GUARD_INTERVAL = 1/16
	HIERARCHY = NONE
	INVERSION = AUTO

