# DVB-T Niedersachsen
# Created from http://www.ueberallfernsehen.de/data/senderliste.pdf
[CH21: NDR NDS, WDR/NDR SH, MDR/NDR MVP, HR/NDR HH]
	DELIVERY_SYSTEM = DVBT
	FREQUENCY = 474000000
	BANDWIDTH_HZ = 8000000
	CODE_RATE_HP = 2/3
	CODE_RATE_LP = NONE
	MODULATION = QAM/16
	TRANSMISSION_MODE = 8K
	GUARD_INTERVAL = 1/4
	HIERARCHY = NONE
	INVERSION = AUTO

[CH22: Das Erste (RB), RB TV (NDR NDS), arte, Phoenix]
	DELIVERY_SYSTEM = DVBT
	FREQUENCY = 482000000
	BANDWIDTH_HZ = 8000000
	CODE_RATE_HP = 2/3
	CODE_RATE_LP = NONE
	MODULATION = QAM/16
	TRANSMISSION_MODE = 8K
	GUARD_INTERVAL = 1/4
	HIERARCHY = NONE
	INVERSION = AUTO

                                            # CH22: Das Erste, arte, Phoenix, EinsExtra
[CH23: ZDF, 3sat, KiKa / ZDFneo, ZDFinfo]
	DELIVERY_SYSTEM = DVBT
	FREQUENCY = 490000000
	BANDWIDTH_HZ = 8000000
	CODE_RATE_HP = 2/3
	CODE_RATE_LP = NONE
	MODULATION = QAM/16
	TRANSMISSION_MODE = 8K
	GUARD_INTERVAL = 1/4
	HIERARCHY = NONE
	INVERSION = AUTO

[CH24: RTL, RTL2, Super RTL, VOX]
	DELIVERY_SYSTEM = DVBT
	FREQUENCY = 498000000
	BANDWIDTH_HZ = 8000000
	CODE_RATE_HP = 2/3
	CODE_RATE_LP = NONE
	MODULATION = QAM/16
	TRANSMISSION_MODE = 8K
	GUARD_INTERVAL = 1/4
	HIERARCHY = NONE
	INVERSION = AUTO

[CH26: Das Erste, arte, Phoenix, EinsExtra]
	DELIVERY_SYSTEM = DVBT
	FREQUENCY = 514000000
	BANDWIDTH_HZ = 8000000
	CODE_RATE_HP = 2/3
	CODE_RATE_LP = NONE
	MODULATION = QAM/16
	TRANSMISSION_MODE = 8K
	GUARD_INTERVAL = 1/4
	HIERARCHY = NONE
	INVERSION = AUTO

[CH28: Tele 5, Nickelodeon/Comedy Central, Eurosport, Mona / Bibel TV / Das Vierte]
	DELIVERY_SYSTEM = DVBT
	FREQUENCY = 530000000
	BANDWIDTH_HZ = 8000000
	CODE_RATE_HP = 2/3
	CODE_RATE_LP = NONE
	MODULATION = QAM/16
	TRANSMISSION_MODE = 8K
	GUARD_INTERVAL = 1/4
	HIERARCHY = NONE
	INVERSION = AUTO

[CH29: NDR NDS, WDR/NDR SH, MDR/NDR MVP, HR/NDR HH]
	DELIVERY_SYSTEM = DVBT
	FREQUENCY = 538000000
	BANDWIDTH_HZ = 8000000
	CODE_RATE_HP = 2/3
	CODE_RATE_LP = NONE
	MODULATION = QAM/16
	TRANSMISSION_MODE = 8K
	GUARD_INTERVAL = 1/4
	HIERARCHY = NONE
	INVERSION = AUTO

[CH31: ZDF, 3sat, KiKa / ZDFneo, ZDFinfo]
	DELIVERY_SYSTEM = DVBT
	FREQUENCY = 554000000
	BANDWIDTH_HZ = 8000000
	CODE_RATE_HP = 2/3
	CODE_RATE_LP = NONE
	MODULATION = QAM/16
	TRANSMISSION_MODE = 8K
	GUARD_INTERVAL = 1/4
	HIERARCHY = NONE
	INVERSION = AUTO

[CH32: ZDF, 3sat, KiKa / ZDFneo, ZDFinfo]
	DELIVERY_SYSTEM = DVBT
	FREQUENCY = 562000000
	BANDWIDTH_HZ = 8000000
	CODE_RATE_HP = 2/3
	CODE_RATE_LP = NONE
	MODULATION = QAM/16
	TRANSMISSION_MODE = 8K
	GUARD_INTERVAL = 1/4
	HIERARCHY = NONE
	INVERSION = AUTO

[CH35: ZDF, 3sat, KiKa / ZDFneo, ZDFinfo]
	DELIVERY_SYSTEM = DVBT
	FREQUENCY = 586000000
	BANDWIDTH_HZ = 8000000
	CODE_RATE_HP = 2/3
	CODE_RATE_LP = NONE
	MODULATION = QAM/16
	TRANSMISSION_MODE = 8K
	GUARD_INTERVAL = 1/4
	HIERARCHY = NONE
	INVERSION = AUTO

[CH36: NDR NDS, WDR/NDR SH, MDR/NDR MVP, HR/NDR HH]
	DELIVERY_SYSTEM = DVBT
	FREQUENCY = 594000000
	BANDWIDTH_HZ = 8000000
	CODE_RATE_HP = 2/3
	CODE_RATE_LP = NONE
	MODULATION = QAM/16
	TRANSMISSION_MODE = 8K
	GUARD_INTERVAL = 1/4
	HIERARCHY = NONE
	INVERSION = AUTO

[CH38: Das Erste, arte, Phoenix, EinsExtra]
	DELIVERY_SYSTEM = DVBT
	FREQUENCY = 610000000
	BANDWIDTH_HZ = 8000000
	CODE_RATE_HP = 2/3
	CODE_RATE_LP = NONE
	MODULATION = QAM/16
	TRANSMISSION_MODE = 8K
	GUARD_INTERVAL = 1/4
	HIERARCHY = NONE
	INVERSION = AUTO

                                            # CH38: ZDF, 3sat, KiKa / ZDFneo, ZDFinfo
[CH42: RTL, RTL2, Super RTL, VOX]
	DELIVERY_SYSTEM = DVBT
	FREQUENCY = 642000000
	BANDWIDTH_HZ = 8000000
	CODE_RATE_HP = 2/3
	CODE_RATE_LP = NONE
	MODULATION = QAM/16
	TRANSMISSION_MODE = 8K
	GUARD_INTERVAL = 1/4
	HIERARCHY = NONE
	INVERSION = AUTO

                                            # CH42: ZDF, 3sat, KiKa / ZDFneo, ZDFinfo
[CH43: Das Erste, arte, Phoenix, EinsExtra]
	DELIVERY_SYSTEM = DVBT
	FREQUENCY = 650000000
	BANDWIDTH_HZ = 8000000
	CODE_RATE_HP = 2/3
	CODE_RATE_LP = NONE
	MODULATION = QAM/16
	TRANSMISSION_MODE = 8K
	GUARD_INTERVAL = 1/4
	HIERARCHY = NONE
	INVERSION = AUTO

                                            # CH43: NDR NDS, WDR/NDR SH, MDR/NDR MVP, HR/NDR HH
[CH44: ProSieben, Sat.1, Kabel1, N24]
	DELIVERY_SYSTEM = DVBT
	FREQUENCY = 658000000
	BANDWIDTH_HZ = 8000000
	CODE_RATE_HP = 2/3
	CODE_RATE_LP = NONE
	MODULATION = QAM/16
	TRANSMISSION_MODE = 8K
	GUARD_INTERVAL = 1/4
	HIERARCHY = NONE
	INVERSION = AUTO

[CH45: Tele 5, SIXX, QVC, Mona / Bibel TV / Das Vierte]
	DELIVERY_SYSTEM = DVBT
	FREQUENCY = 666000000
	BANDWIDTH_HZ = 8000000
	CODE_RATE_HP = 2/3
	CODE_RATE_LP = NONE
	MODULATION = QAM/16
	TRANSMISSION_MODE = 8K
	GUARD_INTERVAL = 1/4
	HIERARCHY = NONE
	INVERSION = AUTO

[CH47: Das Erste, arte, Phoenix, EinsExtra]
	DELIVERY_SYSTEM = DVBT
	FREQUENCY = 682000000
	BANDWIDTH_HZ = 8000000
	CODE_RATE_HP = 2/3
	CODE_RATE_LP = NONE
	MODULATION = QAM/16
	TRANSMISSION_MODE = 8K
	GUARD_INTERVAL = 1/4
	HIERARCHY = NONE
	INVERSION = AUTO

[CH48: Das Erste, arte, Phoenix, EinsExtra]
	DELIVERY_SYSTEM = DVBT
	FREQUENCY = 690000000
	BANDWIDTH_HZ = 8000000
	CODE_RATE_HP = 2/3
	CODE_RATE_LP = NONE
	MODULATION = QAM/16
	TRANSMISSION_MODE = 8K
	GUARD_INTERVAL = 1/4
	HIERARCHY = NONE
	INVERSION = AUTO

[CH49: ProSieben, Sat.1, Kabel1, N24]
	DELIVERY_SYSTEM = DVBT
	FREQUENCY = 698000000
	BANDWIDTH_HZ = 8000000
	CODE_RATE_HP = 2/3
	CODE_RATE_LP = NONE
	MODULATION = QAM/16
	TRANSMISSION_MODE = 8K
	GUARD_INTERVAL = 1/4
	HIERARCHY = NONE
	INVERSION = AUTO

[CH58: NDR NDS, WDR/NDR SH, MDR/NDR MVP, HR/NDR HH]
	DELIVERY_SYSTEM = DVBT
	FREQUENCY = 770000000
	BANDWIDTH_HZ = 8000000
	CODE_RATE_HP = 2/3
	CODE_RATE_LP = NONE
	MODULATION = QAM/16
	TRANSMISSION_MODE = 8K
	GUARD_INTERVAL = 1/4
	HIERARCHY = NONE
	INVERSION = AUTO

[CH59: Das Erste, arte, Phoenix, EinsExtra]
	DELIVERY_SYSTEM = DVBT
	FREQUENCY = 778000000
	BANDWIDTH_HZ = 8000000
	CODE_RATE_HP = 2/3
	CODE_RATE_LP = NONE
	MODULATION = QAM/16
	TRANSMISSION_MODE = 8K
	GUARD_INTERVAL = 1/4
	HIERARCHY = NONE
	INVERSION = AUTO

[CH60: Tele 5, Nickelodeon/Comedy Central, Eurosport, Mona / Bibel TV / Das Vierte]
	DELIVERY_SYSTEM = DVBT
	FREQUENCY = 786000000
	BANDWIDTH_HZ = 8000000
	CODE_RATE_HP = 2/3
	CODE_RATE_LP = NONE
	MODULATION = QAM/16
	TRANSMISSION_MODE = 8K
	GUARD_INTERVAL = 1/4
	HIERARCHY = NONE
	INVERSION = AUTO

