# Australia / NSW / New England / Tamworth / Mt.Soma
# SBS
[CHANNEL]
	DELIVERY_SYSTEM = DVBT
	FREQUENCY = 690500000
	BANDWIDTH_HZ = 7000000
	CODE_RATE_HP = 2/3
	CODE_RATE_LP = NONE
	MODULATION = QAM/64
	TRANSMISSION_MODE = 8K
	GUARD_INTERVAL = 1/8
	HIERARCHY = NONE
	INVERSION = AUTO

# NBN
[CHANNEL]
	DELIVERY_SYSTEM = DVBT
	FREQUENCY = 753500000
	BANDWIDTH_HZ = 7000000
	CODE_RATE_HP = 3/4
	CODE_RATE_LP = NONE
	MODULATION = QAM/64
	TRANSMISSION_MODE = 8K
	GUARD_INTERVAL = 1/16
	HIERARCHY = NONE
	INVERSION = AUTO

# Prime
[CHANNEL]
	DELIVERY_SYSTEM = DVBT
	FREQUENCY = 732500000
	BANDWIDTH_HZ = 7000000
	CODE_RATE_HP = 3/4
	CODE_RATE_LP = NONE
	MODULATION = QAM/64
	TRANSMISSION_MODE = 8K
	GUARD_INTERVAL = 1/16
	HIERARCHY = NONE
	INVERSION = AUTO

# ABC
[CHANNEL]
	DELIVERY_SYSTEM = DVBT
	FREQUENCY = 711500000
	BANDWIDTH_HZ = 7000000
	CODE_RATE_HP = 3/4
	CODE_RATE_LP = NONE
	MODULATION = QAM/64
	TRANSMISSION_MODE = 8K
	GUARD_INTERVAL = 1/16
	HIERARCHY = NONE
	INVERSION = AUTO

# SC10
[CHANNEL]
	DELIVERY_SYSTEM = DVBT
	FREQUENCY = 774500000
	BANDWIDTH_HZ = 7000000
	CODE_RATE_HP = 3/4
	CODE_RATE_LP = NONE
	MODULATION = QAM/64
	TRANSMISSION_MODE = 8K
	GUARD_INTERVAL = 1/16
	HIERARCHY = NONE
	INVERSION = AUTO


# Australia / NSW / New England / Upper Namoi / Mt.Dowe
# SBS
[CHANNEL]
	DELIVERY_SYSTEM = DVBT
	FREQUENCY = 585500000
	BANDWIDTH_HZ = 7000000
	CODE_RATE_HP = 2/3
	CODE_RATE_LP = NONE
	MODULATION = QAM/64
	TRANSMISSION_MODE = 8K
	GUARD_INTERVAL = 1/8
	HIERARCHY = NONE
	INVERSION = AUTO

# NBN
[CHANNEL]
	DELIVERY_SYSTEM = DVBT
	FREQUENCY = 592500000
	BANDWIDTH_HZ = 7000000
	CODE_RATE_HP = 3/4
	CODE_RATE_LP = NONE
	MODULATION = QAM/64
	TRANSMISSION_MODE = 8K
	GUARD_INTERVAL = 1/16
	HIERARCHY = NONE
	INVERSION = AUTO

# Prime
[CHANNEL]
	DELIVERY_SYSTEM = DVBT
	FREQUENCY = 205625000
	BANDWIDTH_HZ = 7000000
	CODE_RATE_HP = 3/4
	CODE_RATE_LP = NONE
	MODULATION = QAM/64
	TRANSMISSION_MODE = 8K
	GUARD_INTERVAL = 1/16
	HIERARCHY = NONE
	INVERSION = AUTO

# ABC
[CHANNEL]
	DELIVERY_SYSTEM = DVBT
	FREQUENCY = 191625000
	BANDWIDTH_HZ = 7000000
	CODE_RATE_HP = 3/4
	CODE_RATE_LP = NONE
	MODULATION = QAM/64
	TRANSMISSION_MODE = 8K
	GUARD_INTERVAL = 1/16
	HIERARCHY = NONE
	INVERSION = AUTO

# SC10
[CHANNEL]
	DELIVERY_SYSTEM = DVBT
	FREQUENCY = 613500000
	BANDWIDTH_HZ = 7000000
	CODE_RATE_HP = 3/4
	CODE_RATE_LP = NONE
	MODULATION = QAM/64
	TRANSMISSION_MODE = 8K
	GUARD_INTERVAL = 1/16
	HIERARCHY = NONE
	INVERSION = AUTO


# Australia / NSW / Western Districts / Central Western Slopes / Mt. Cenn Cruaich
# SBS
[CHANNEL]
	DELIVERY_SYSTEM = DVBT
	FREQUENCY = 641500000
	BANDWIDTH_HZ = 7000000
	CODE_RATE_HP = 2/3
	CODE_RATE_LP = NONE
	MODULATION = QAM/64
	TRANSMISSION_MODE = 8K
	GUARD_INTERVAL = 1/8
	HIERARCHY = NONE
	INVERSION = AUTO

# WIN
[CHANNEL]
	DELIVERY_SYSTEM = DVBT
	FREQUENCY = 648500000
	BANDWIDTH_HZ = 7000000
	CODE_RATE_HP = 3/4
	CODE_RATE_LP = NONE
	MODULATION = QAM/64
	TRANSMISSION_MODE = 8K
	GUARD_INTERVAL = 1/16
	HIERARCHY = NONE
	INVERSION = AUTO

# Prime
[CHANNEL]
	DELIVERY_SYSTEM = DVBT
	FREQUENCY = 620500000
	BANDWIDTH_HZ = 7000000
	CODE_RATE_HP = 3/4
	CODE_RATE_LP = NONE
	MODULATION = QAM/64
	TRANSMISSION_MODE = 8K
	GUARD_INTERVAL = 1/16
	HIERARCHY = NONE
	INVERSION = AUTO

# ABC
[CHANNEL]
	DELIVERY_SYSTEM = DVBT
	FREQUENCY = 226625000
	BANDWIDTH_HZ = 7000000
	CODE_RATE_HP = 3/4
	CODE_RATE_LP = NONE
	MODULATION = QAM/64
	TRANSMISSION_MODE = 8K
	GUARD_INTERVAL = 1/16
	HIERARCHY = NONE
	INVERSION = AUTO

# SC10
[CHANNEL]
	DELIVERY_SYSTEM = DVBT
	FREQUENCY = 641500000
	BANDWIDTH_HZ = 7000000
	CODE_RATE_HP = 3/4
	CODE_RATE_LP = NONE
	MODULATION = QAM/64
	TRANSMISSION_MODE = 8K
	GUARD_INTERVAL = 1/16
	HIERARCHY = NONE
	INVERSION = AUTO

