# Ireland, Spur Hill
# Generated from http://www.comreg.ie/_fileupload/Broadcast_Technical_Parameters.xlsx
[CH45: Saorview MUX1]
	DELIVERY_SYSTEM = DVBT
	FREQUENCY = 666000000
	BANDWIDTH_HZ = 8000000
	CODE_RATE_HP = 3/4
	CODE_RATE_LP = NONE
	MODULATION = QAM/64
	TRANSMISSION_MODE = 8K
	GUARD_INTERVAL = 1/32
	HIERARCHY = NONE
	INVERSION = AUTO

[CH49: Saorview MUX2]
	DELIVERY_SYSTEM = DVBT
	FREQUENCY = 698000000
	BANDWIDTH_HZ = 8000000
	CODE_RATE_HP = 3/4
	CODE_RATE_LP = NONE
	MODULATION = QAM/64
	TRANSMISSION_MODE = 8K
	GUARD_INTERVAL = 1/32
	HIERARCHY = NONE
	INVERSION = AUTO

