# Ireland, Three Rock
# Generated from http://www.comreg.ie/_fileupload/Broadcast_Technical_Parameters.xlsx
[CH30: Saorview MUX1]
	DELIVERY_SYSTEM = DVBT
	FREQUENCY = 546000000
	BANDWIDTH_HZ = 8000000
	CODE_RATE_HP = 3/4
	CODE_RATE_LP = NONE
	MODULATION = QAM/16
	TRANSMISSION_MODE = 2K
	GUARD_INTERVAL = 1/32
	HIERARCHY = NONE
	INVERSION = AUTO

[CH33: Saorview MUX2]
	DELIVERY_SYSTEM = DVBT
	FREQUENCY = 570000000
	BANDWIDTH_HZ = 8000000
	CODE_RATE_HP = 3/4
	CODE_RATE_LP = NONE
	MODULATION = QAM/16
	TRANSMISSION_MODE = 2K
	GUARD_INTERVAL = 1/32
	HIERARCHY = NONE
	INVERSION = AUTO

