# Initial scan config for Swiss DVB-C provider Quickline in Aarberg (EWA)
[CHANNEL]
	DELIVERY_SYSTEM = DVBC/ANNEX_A
	FREQUENCY = 306000000
	SYMBOL_RATE = 6900000
	INNER_FEC = NONE
	MODULATION = QAM/256
	INVERSION = AUTO
