Add extra debug for the q_d_w_o() when work fn is already active.

From: Paul Walmsley <paul@pwsan.com>


---

 arch/arm/mach-omap2/timer-gp.c      |    3 ++-
 arch/arm/plat-omap/dmtimer.c        |   20 ++++++++++++++++++++
 include/asm-arm/arch-omap/dmtimer.h |    1 +
 kernel/time/timer_list.c            |    8 ++++++++
 4 files changed, 31 insertions(+), 1 deletions(-)

diff --git a/arch/arm/mach-omap2/timer-gp.c b/arch/arm/mach-omap2/timer-gp.c
index ce5c2b4..e3ed368 100644
--- a/arch/arm/mach-omap2/timer-gp.c
+++ b/arch/arm/mach-omap2/timer-gp.c
@@ -50,6 +50,7 @@
 #define GPTIMER_MATCH_VAL	(0xffffffff - (32768/2))
 
 static struct omap_dm_timer *gptimer;
+struct omap_dm_timer *gptimer_pub;
 static struct clock_event_device clockevent_gpt;
 
 static u32 last_load;
@@ -111,7 +112,7 @@ static void __init omap2_gp_clockevent_init(void)
 {
 	u32 tick_rate;
 
-	gptimer = omap_dm_timer_request_specific(1);
+	gptimer = gptimer_pub = omap_dm_timer_request_specific(1);
 	BUG_ON(gptimer == NULL);
 
 #if defined(CONFIG_OMAP_32K_TIMER)
diff --git a/arch/arm/plat-omap/dmtimer.c b/arch/arm/plat-omap/dmtimer.c
index e38a11e..b10f8ac 100644
--- a/arch/arm/plat-omap/dmtimer.c
+++ b/arch/arm/plat-omap/dmtimer.c
@@ -614,6 +614,26 @@ void omap_dm_timer_set_int_enable(struct omap_dm_timer *timer,
 	omap_dm_timer_write_reg(timer, OMAP_TIMER_WAKEUP_EN_REG, value);
 }
 
+void omap_dm_timer_dump_int_enable(struct omap_dm_timer *timer)
+{
+	u32 l;
+	l = omap_dm_timer_read_reg(timer, OMAP_TIMER_COUNTER_REG);
+	pr_err("GPT TCRR: %08x\n", l);
+	l = omap_dm_timer_read_reg(timer, OMAP_TIMER_MATCH_REG);
+	pr_err("GPT TMAT: %08x\n", l);
+	l = omap_dm_timer_read_reg(timer, OMAP_TIMER_STAT_REG);
+	pr_err("GPT TISR: %08x\n", l);
+	l = omap_dm_timer_read_reg(timer, OMAP_TIMER_INT_EN_REG);
+	pr_err("GPT TIER: %08x\n", l);
+	l = omap_dm_timer_read_reg(timer, OMAP_TIMER_CTRL_REG);
+	pr_err("GPT TCLR: %08x\n", l);
+	l = omap_dm_timer_read_reg(timer, OMAP_TIMER_TICK_INT_MASK_SET_REG);
+	pr_err("GPT TOCR: %08x\n", l);
+	l = omap_dm_timer_read_reg(timer, OMAP_TIMER_TICK_INT_MASK_COUNT_REG);
+	pr_err("GPT TOWR: %08x\n", l);
+}
+
+
 unsigned int omap_dm_timer_read_status(struct omap_dm_timer *timer)
 {
 	unsigned int l;
diff --git a/include/asm-arm/arch-omap/dmtimer.h b/include/asm-arm/arch-omap/dmtimer.h
index 02b29e8..a8123e9 100644
--- a/include/asm-arm/arch-omap/dmtimer.h
+++ b/include/asm-arm/arch-omap/dmtimer.h
@@ -73,6 +73,7 @@ void omap_dm_timer_set_prescaler(struct omap_dm_timer *timer, int prescaler);
 
 void omap_dm_timer_set_int_enable(struct omap_dm_timer *timer, unsigned int value);
 
+void omap_dm_timer_dump_int_enable(struct omap_dm_timer *timer);
 unsigned int omap_dm_timer_read_status(struct omap_dm_timer *timer);
 void omap_dm_timer_write_status(struct omap_dm_timer *timer, unsigned int value);
 unsigned int omap_dm_timer_read_counter(struct omap_dm_timer *timer);
diff --git a/kernel/time/timer_list.c b/kernel/time/timer_list.c
index a40e20f..452eab7 100644
--- a/kernel/time/timer_list.c
+++ b/kernel/time/timer_list.c
@@ -18,6 +18,8 @@
 #include <linux/kallsyms.h>
 #include <linux/tick.h>
 
+#include <asm/arch/dmtimer.h>
+
 #include <asm/uaccess.h>
 
 typedef void (*print_fn_t)(struct seq_file *m, unsigned int *classes);
@@ -239,6 +241,8 @@ static void timer_list_show_tickdevices(struct seq_file *m)
 static void timer_list_show_tickdevices(struct seq_file *m) { }
 #endif
 
+extern struct omap_dm_timer *gptimer_pub;
+
 static int timer_list_show(struct seq_file *m, void *v)
 {
 	u64 now = ktime_to_ns(ktime_get());
@@ -254,6 +258,10 @@ static int timer_list_show(struct seq_file *m, void *v)
 	SEQ_printf(m, "\n");
 	timer_list_show_tickdevices(m);
 
+	SEQ_printf(m, "\n");
+	
+	omap_dm_timer_dump_int_enable(gptimer_pub);
+
 	return 0;
 }
 
