---
 arch/arm/mach-mx3/mx31lite.c     |   26 ++++++++++++++++++++++++++
 drivers/video/mxc/mxcfb_modedb.c |   25 +++++++++++++++++++++++++
 2 files changed, 51 insertions(+)

Index: linux-2.6.19.2/arch/arm/mach-mx3/mx31lite.c
===================================================================
--- linux-2.6.19.2.orig/arch/arm/mach-mx3/mx31lite.c	2007-10-03 19:37:43.000000000 +0200
+++ linux-2.6.19.2/arch/arm/mach-mx3/mx31lite.c	2007-10-03 19:43:09.000000000 +0200
@@ -280,6 +280,31 @@
 }
 #endif
 
+#if defined(CONFIG_FB_MXC_SYNC_PANEL) || defined(CONFIG_FB_MXC_SYNC_PANEL_MODULE)
+static const char fb_default_mode[] = "Sharpsix-VGA";
+
+/* mxc lcd driver */
+static struct platform_device mxc_fb_device = {
+	.name = "mxc_sdc_fb",
+	.id = 0,
+	.dev = {
+		.release = mxc_nop_release,
+		.platform_data = &fb_default_mode,
+		.coherent_dma_mask = 0xFFFFFFFF,
+		},
+};
+
+static void mxc_init_fb(void)
+{
+	(void)platform_device_register(&mxc_fb_device);
+}
+#else
+static inline void mxc_init_fb(void)
+{
+}
+#endif
+
+
 /*!
  * Board specific fixup function. It is called by \b setup_arch() in
  * setup.c file very early on during kernel starts. It allows the user to
@@ -400,6 +425,7 @@
 	mxc_init_nor_mtd();
 	mxc_init_nand_mtd();
 	mxc_init_eth();
+	mxc_init_fb();
 }
 
 /*
Index: linux-2.6.19.2/drivers/video/mxc/mxcfb_modedb.c
===================================================================
--- linux-2.6.19.2.orig/drivers/video/mxc/mxcfb_modedb.c	2007-10-03 19:37:43.000000000 +0200
+++ linux-2.6.19.2/drivers/video/mxc/mxcfb_modedb.c	2007-10-03 19:43:02.000000000 +0200
@@ -55,6 +55,31 @@
 	       "TV-VGA", 60, 640, 480, 40574, 35, 45, 9, 1, 46, 5,
 	       0, FB_VMODE_NONINTERLACED, 0,
 	       },
+	[5] = {
+		/* 640x480 @ 60 Hz, 6" */
+		"Sharpsix-VGA",
+		60, 640, 480,   // 60 Hz, 640x480
+		35285,      // 36.66 ns clock period
+		128, 128,   // left & right margin
+		34, 10,      // upper & lower margin
+		2, 2,      // hsync & vsync len
+		FB_SYNC_OE_ACT_HIGH,
+		FB_VMODE_NONINTERLACED,
+		0,
+	},
+	[6] = {
+		/* 640x480 @ 60 Hz 10" */
+		"Sharpten-VGA",
+		60, 640, 480,   // 60 Hz, 640x480
+		35285,      // 35.285b ns clock period
+		128, 128,   // left & right margin
+		34, 10,      // upper & lower margin
+		2, 2,      // hsync & vsync len
+		FB_SYNC_OE_ACT_HIGH,
+		FB_VMODE_NONINTERLACED,
+		0,
+	},
+
 };
 
 int mxcfb_modedb_sz = ARRAY_SIZE(mxcfb_modedb);
