# This file lists the configuration options that are used when building the
# hostapd binary. All lines starting with # are ignored. Configuration option
# lines must be commented out complete, if they are not to be included, i.e.,
# just setting VARIABLE=n is not disabling that variable.
#
# This file is included in Makefile, so variables like CFLAGS and LIBS can also
# be modified from here. In most cass, these lines should use += in order not
# to override previous values of the variables.

CFLAGS = $(TARGET_CFLAGS) -I../src/hostapd -I../src/utils -I../src/driver/modules -I../src/rsn_supp -I../src/common -I../src/crypto -I../src -I./ -Wall -MMD
LIBS = $(TARGET_LDFLAGS)

# Driver interface for Host AP driver
CONFIG_DRIVER_HOSTAP=y

# Driver interface for Agere driver
#CONFIG_DRIVER_HERMES=y
#CFLAGS += -I../../hcf -I../../include -I../../include/hcf

# Driver interface for madwifi driver
#CONFIG_DRIVER_MADWIFI=y
#CFLAGS += -I../madwifi/wpa

# Driver interface for Prism54 driver
#CONFIG_DRIVER_PRISM54=y

# Driver interface for ndiswrapper
#CONFIG_DRIVER_NDISWRAPPER=y

# Driver interface for Atmel driver
#CONFIG_DRIVER_ATMEL=y

# Driver interface for Broadcom driver
#CONFIG_DRIVER_BROADCOM=y
#CFLAGS += -I/opt/WRT54GS/release/src/include

# Driver interface for Intel ipw2100 driver
#CONFIG_DRIVER_IPW2100=y

# Driver interface for generic Linux wireless extensions
CONFIG_DRIVER_WEXT=y

# Driver interface for FreeBSD net80211 layer (e.g., Atheros driver)
#CONFIG_DRIVER_BSD=y
#CFLAGS += -I/usr/local/include
#LIBS += -L/usr/local/lib

# Driver interface for development testing
#CONFIG_DRIVER_TEST=y

# Driver interface for wired Ethernet drivers
CONFIG_DRIVER_WIRED=y

# Enable IEEE 802.1X Supplicant (automatically included if any EAP method is
# included)
CONFIG_IEEE8021X_EAPOL=y

# EAP-MD5 (automatically included if EAP-TTLS is enabled)
CONFIG_EAP_MD5=y

# EAP-MSCHAPv2 (automatically included if EAP-PEAP is enabled)
CONFIG_EAP_MSCHAPV2=y

# EAP-TLS
CONFIG_EAP_TLS=y

# EAL-PEAP
CONFIG_EAP_PEAP=y

# EAP-TTLS
CONFIG_EAP_TTLS=y

# EAP-GTC
CONFIG_EAP_GTC=y

# EAP-OTP
CONFIG_EAP_OTP=y

# EAP-SIM (enable CONFIG_PCSC, if EAP-SIM is used)
#CONFIG_EAP_SIM=y

# EAP-PSK (experimental; this is _not_ needed for WPA-PSK)
#CONFIG_EAP_PSK=y

# EAP-PAX
#CONFIG_EAP_PAX=y

# LEAP
CONFIG_EAP_LEAP=y

# EAP-AKA (enable CONFIG_PCSC, if EAP-AKA is used)
#CONFIG_EAP_AKA=y

# PKCS#12 (PFX) support (used to read private key and certificate file from
# a file that usually has extension .p12 or .pfx)
CONFIG_PKCS12=y

# Smartcard support (i.e., private key on a smartcard), e.g., with openssl
# engine.
CONFIG_SMARTCARD=y

# PC/SC interface for smartcards (USIM, GSM SIM)
# Enable this if EAP-SIM or EAP-AKA is included
#CONFIG_PCSC=y

# Development testing
#CONFIG_EAPOL_TEST=y

# Replace native Linux implementation of packet sockets with libdnet/libpcap.
# This will be automatically set for non-Linux OS.
#CONFIG_DNET_PCAP=y

# Include control interface for external programs, e.g, wpa_cli
CONFIG_CTRL_IFACE=y

# Include support for GNU Readline and History Libraries in wpa_cli.
# When building a wpa_cli binary for distribution, please note that these
# libraries are licensed under GPL and as such, BSD license may not apply for
# the resulting binary.
#CONFIG_READLINE=y

# Remove debugging code that is printing out debug message to stdout.
# This can be used to reduce the size of the wpa_supplicant considerably
# if debugging code is not needed. The size reduction can be around 35%
# (e.g., 90 kB).
#CONFIG_NO_STDOUT_DEBUG=y

# Remove WPA support, e.g., for wired-only IEEE 802.1X supplicant, to save
# 35-50 kB in code size.
#CONFIG_NO_WPA=y

# Select configuration backend:
# file = text file (e.g., wpa_supplicant.conf)
# winreg = Windows registry (see win_example.reg for an example)
CONFIG_BACKEND=file

# Select program entry point implementation:
# main = UNIX/POSIX like main() function (default)
# main_winsvc = Windows service (read parameters from registry)
# main_none = Very basic example (development use only)
#CONFIG_MAIN=main

# Select wrapper for operatins system and C library specific functions
# unix = UNIX/POSIX like systems (default)
# win32 = Windows systems
# none = Empty template
#CONFIG_OS=unix

# Select event loop implementation
# eloop = select() loop (default)
# eloop_win = Windows events and WaitForMultipleObject() loop
# eloop_none = Empty template
#CONFIG_ELOOP=eloop

# Select layer 2 packet implementation
# linux = Linux packet socket (default)
# pcap = libpcap/libdnet/WinPcap
# freebsd = FreeBSD libpcap
# winpcap = WinPcap with receive thread
# none = Empty template
#CONFIG_L2_PACKET=linux

# IEEE 802.11i/IEEE 802.11e STAKey negotiation for direct link connection
#CONFIG_STAKEY=y

# Select TLS implementation
# openssl = OpenSSL (default)
# gnutls = GnuTLS (needed for TLS/IA, see also CONFIG_GNUTLS_EXTRA)
# none = Empty template
CONFIG_TLS=gnutls

# Whether to enable TLS/IA support, which is required for EAP-TTLSv1.
# You need CONFIG_TLS=gnutls for this to have any effect. Please note that
# even though the core GnuTLS library is released under LGPL, this extra
# library uses GPL and as such, the terms of GPL apply to the combination
# of wpa_supplicant and GnuTLS if this option is enabled. BSD license may not
# apply for distribution of the resulting binary.
CONFIG_GNUTLS_EXTRA=y

CONFIG_CTRL_IFACE_DBUS=y
