# Australia / Tasmania / Devonport
#
# Brett S Hallett October 2009 , may not be complete !!
#
# ABC VHF 57
[CHANNEL]
	DELIVERY_SYSTEM = DVBT
	FREQUENCY = 730250000
	BANDWIDTH_HZ = 7000000
	CODE_RATE_HP = 3/4
	CODE_RATE_LP = NONE
	MODULATION = QAM/64
	TRANSMISSION_MODE = 8K
	GUARD_INTERVAL = 1/16
	HIERARCHY = NONE
	INVERSION = AUTO

# ABC Digital 45
[CHANNEL]
	DELIVERY_SYSTEM = DVBT
	FREQUENCY = 648500000
	BANDWIDTH_HZ = 7000000
	CODE_RATE_HP = 3/4
	CODE_RATE_LP = NONE
	MODULATION = QAM/64
	TRANSMISSION_MODE = 8K
	GUARD_INTERVAL = 1/16
	HIERARCHY = NONE
	INVERSION = AUTO

# SBS VHF 54
[CHANNEL]
	DELIVERY_SYSTEM = DVBT
	FREQUENCY = 709250000
	BANDWIDTH_HZ = 7000000
	CODE_RATE_HP = 2/3
	CODE_RATE_LP = NONE
	MODULATION = QAM/64
	TRANSMISSION_MODE = 8K
	GUARD_INTERVAL = 1/8
	HIERARCHY = NONE
	INVERSION = AUTO

# SBS Digital 39
[CHANNEL]
	DELIVERY_SYSTEM = DVBT
	FREQUENCY = 606500000
	BANDWIDTH_HZ = 7000000
	CODE_RATE_HP = 2/3
	CODE_RATE_LP = NONE
	MODULATION = QAM/64
	TRANSMISSION_MODE = 8K
	GUARD_INTERVAL = 1/8
	HIERARCHY = NONE
	INVERSION = AUTO

# SCTV
[CHANNEL]
	DELIVERY_SYSTEM = DVBT
	FREQUENCY = 613498000
	BANDWIDTH_HZ = 7000000
	CODE_RATE_HP = 3/4
	CODE_RATE_LP = NONE
	MODULATION = QAM/64
	TRANSMISSION_MODE = 8K
	GUARD_INTERVAL = 1/16
	HIERARCHY = NONE
	INVERSION = AUTO

# WIN
[CHANNEL]
	DELIVERY_SYSTEM = DVBT
	FREQUENCY = 627498000
	BANDWIDTH_HZ = 7000000
	CODE_RATE_HP = 3/4
	CODE_RATE_LP = NONE
	MODULATION = QAM/64
	TRANSMISSION_MODE = 8K
	GUARD_INTERVAL = 1/8
	HIERARCHY = NONE
	INVERSION = AUTO

# TDT
[CHANNEL]
	DELIVERY_SYSTEM = DVBT
	FREQUENCY = 585498000
	BANDWIDTH_HZ = 7000000
	CODE_RATE_HP = 2/3
	CODE_RATE_LP = NONE
	MODULATION = QAM/64
	TRANSMISSION_MODE = 8K
	GUARD_INTERVAL = 1/8
	HIERARCHY = NONE
	INVERSION = AUTO

