# DVB-T Sachsen
# Created from http://www.ueberallfernsehen.de/data/senderliste.pdf
[CH22: ZDF, 3sat, KiKa / ZDFneo, ZDFinfo]
	DELIVERY_SYSTEM = DVBT
	FREQUENCY = 482000000
	BANDWIDTH_HZ = 8000000
	CODE_RATE_HP = 2/3
	CODE_RATE_LP = NONE
	MODULATION = QAM/16
	TRANSMISSION_MODE = 8K
	GUARD_INTERVAL = 1/4
	HIERARCHY = NONE
	INVERSION = AUTO

[CH24: Das Erste, arte, Phoenix, EinsFestival]
	DELIVERY_SYSTEM = DVBT
	FREQUENCY = 498000000
	BANDWIDTH_HZ = 8000000
	CODE_RATE_HP = 2/3
	CODE_RATE_LP = NONE
	MODULATION = QAM/64
	TRANSMISSION_MODE = 8K
	GUARD_INTERVAL = 1/4
	HIERARCHY = NONE
	INVERSION = AUTO

[CH25: Das Erste, arte, Phoenix, EinsFestival]
	DELIVERY_SYSTEM = DVBT
	FREQUENCY = 506000000
	BANDWIDTH_HZ = 8000000
	CODE_RATE_HP = 2/3
	CODE_RATE_LP = NONE
	MODULATION = QAM/64
	TRANSMISSION_MODE = 8K
	GUARD_INTERVAL = 1/4
	HIERARCHY = NONE
	INVERSION = AUTO

[CH27: MDR-SN, rbb, Bayerisches Fernsehen, WDR]
	DELIVERY_SYSTEM = DVBT
	FREQUENCY = 522000000
	BANDWIDTH_HZ = 8000000
	CODE_RATE_HP = 2/3
	CODE_RATE_LP = NONE
	MODULATION = QAM/64
	TRANSMISSION_MODE = 8K
	GUARD_INTERVAL = 1/4
	HIERARCHY = NONE
	INVERSION = AUTO

[CH28: RTL, RTL2, Super RTL, VOX, RTL Crime, Passion [Sendenorm: MPEG-4]]
	DELIVERY_SYSTEM = DVBT
	FREQUENCY = 530000000
	BANDWIDTH_HZ = 8000000
	CODE_RATE_HP = 3/4
	CODE_RATE_LP = NONE
	MODULATION = QAM/16
	TRANSMISSION_MODE = 8K
	GUARD_INTERVAL = 1/8
	HIERARCHY = NONE
	INVERSION = AUTO

[CH29: MDR-SN, rbb, Bayerisches Fernsehen, WDR]
	DELIVERY_SYSTEM = DVBT
	FREQUENCY = 538000000
	BANDWIDTH_HZ = 8000000
	CODE_RATE_HP = 2/3
	CODE_RATE_LP = NONE
	MODULATION = QAM/64
	TRANSMISSION_MODE = 8K
	GUARD_INTERVAL = 1/4
	HIERARCHY = NONE
	INVERSION = AUTO

[CH31: LF Leipzg.Ferns., InfoTVLeipzig, BBCWorld, Bibel.TV, RadioLeipzig, RadioHoreb]
	DELIVERY_SYSTEM = DVBT
	FREQUENCY = 554000000
	BANDWIDTH_HZ = 8000000
	CODE_RATE_HP = 2/3
	CODE_RATE_LP = NONE
	MODULATION = QAM/16
	TRANSMISSION_MODE = 8K
	GUARD_INTERVAL = 1/16
	HIERARCHY = NONE
	INVERSION = AUTO

[CH32: MDR-SN, rbb, Bayerisches Fernsehen, WDR]
	DELIVERY_SYSTEM = DVBT
	FREQUENCY = 562000000
	BANDWIDTH_HZ = 8000000
	CODE_RATE_HP = 2/3
	CODE_RATE_LP = NONE
	MODULATION = QAM/64
	TRANSMISSION_MODE = 8K
	GUARD_INTERVAL = 1/4
	HIERARCHY = NONE
	INVERSION = AUTO

[CH36: ZDF, 3sat, KiKa / ZDFneo, ZDFinfo]
	DELIVERY_SYSTEM = DVBT
	FREQUENCY = 594000000
	BANDWIDTH_HZ = 8000000
	CODE_RATE_HP = 2/3
	CODE_RATE_LP = NONE
	MODULATION = QAM/16
	TRANSMISSION_MODE = 8K
	GUARD_INTERVAL = 1/4
	HIERARCHY = NONE
	INVERSION = AUTO

[CH37: MDR-SN, rbb, Bayerisches Fernsehen, WDR]
	DELIVERY_SYSTEM = DVBT
	FREQUENCY = 602000000
	BANDWIDTH_HZ = 8000000
	CODE_RATE_HP = 2/3
	CODE_RATE_LP = NONE
	MODULATION = QAM/64
	TRANSMISSION_MODE = 8K
	GUARD_INTERVAL = 1/4
	HIERARCHY = NONE
	INVERSION = AUTO

[CH39: Das Erste, arte, Phoenix, EinsFestival]
	DELIVERY_SYSTEM = DVBT
	FREQUENCY = 618000000
	BANDWIDTH_HZ = 8000000
	CODE_RATE_HP = 2/3
	CODE_RATE_LP = NONE
	MODULATION = QAM/64
	TRANSMISSION_MODE = 8K
	GUARD_INTERVAL = 1/4
	HIERARCHY = NONE
	INVERSION = AUTO

