SUMMARY = "Connman config to ignore wired interface on qemu machines"
DESCRIPTION = "This is the ConnMan configuration to avoid touching wired \
network interface inside qemu machines."
LICENSE = "GPL-2.0-only"
LIC_FILES_CHKSUM = "file://${COREBASE}/meta/files/common-licenses/GPL-2.0-only;md5=801f80980d171dd6425610833a22dbe6"

SRC_URI = "file://main.conf \
          "

S = "${UNPACKDIR}"

PACKAGE_ARCH = "${MACHINE_ARCH}"

FILES:${PN} = "${sysconfdir}/*"

# Kernel IP-Config is perfectly capable of setting up networking passed in via ip=
do_install:append:qemuall() {
    mkdir -p ${D}${sysconfdir}/connman
    cp ${S}/main.conf ${D}${sysconfdir}/connman/main.conf
}
