7/30/2010 - rebased to 3.1.5 by Qing He <qing.he@intel.com>

diff -uNr pciutils-3.1.5.orig/Makefile pciutils-3.1.5/Makefile
--- pciutils-3.1.5.orig/Makefile	2010-07-30 14:02:15.000000000 +0800
+++ pciutils-3.1.5/Makefile	2010-07-30 14:02:55.000000000 +0800
@@ -51,7 +51,7 @@
 
 export
 
-all: lib/$(PCILIB) lspci setpci example lspci.8 setpci.8 pcilib.7 update-pciids update-pciids.8 $(PCI_IDS)
+all: lib/$(PCILIB) lspci setpci example lspci.8 setpci.8 pcilib.7 update-pciids update-pciids.8 $(PCI_IDS) pcimodules pcimodules.8
 
 lib/$(PCILIB): $(PCIINC) force
 	$(MAKE) -C lib all
@@ -61,9 +61,11 @@
 lib/config.h lib/config.mk:
 	cd lib && ./configure
 
+pcimodules: pcimodules.o common.o lib/$(PCILIB)
 lspci: lspci.o ls-vpd.o ls-caps.o ls-ecaps.o ls-kernel.o ls-tree.o ls-map.o common.o lib/$(PCILIB)
 setpci: setpci.o common.o lib/$(PCILIB)
 
+pcimodules.o: pcimodules.c pciutils.h
 LSPCIINC=lspci.h pciutils.h $(PCIINC)
 lspci.o: lspci.c $(LSPCIINC)
 ls-vpd.o: ls-vpd.c $(LSPCIINC)
@@ -100,10 +102,10 @@
 install: all
 # -c is ignored on Linux, but required on FreeBSD
 	$(DIRINSTALL) -m 755 $(DESTDIR)$(SBINDIR) $(DESTDIR)$(IDSDIR) $(DESTDIR)$(MANDIR)/man8 $(DESTDIR)$(MANDIR)/man7
-	$(INSTALL) -c -m 755 lspci setpci $(DESTDIR)$(SBINDIR)
+	$(INSTALL) -c -m 755 lspci setpci pcimodules $(DESTDIR)$(SBINDIR)
 	$(INSTALL) -c -m 755 update-pciids $(DESTDIR)$(SBINDIR)
 	$(INSTALL) -c -m 644 $(PCI_IDS) $(DESTDIR)$(IDSDIR)
-	$(INSTALL) -c -m 644 lspci.8 setpci.8 update-pciids.8 $(DESTDIR)$(MANDIR)/man8
+	$(INSTALL) -c -m 644 lspci.8 setpci.8 update-pciids.8 pcimodules.8 $(DESTDIR)$(MANDIR)/man8
 	$(INSTALL) -c -m 644 pcilib.7 $(DESTDIR)$(MANDIR)/man7
 ifeq ($(SHARED),yes)
 	$(DIRINSTALL) -m 755 $(DESTDIR)$(LIBDIR)
@@ -121,9 +123,9 @@
 endif
 
 uninstall: all
-	rm -f $(DESTDIR)$(SBINDIR)/lspci $(DESTDIR)$(SBINDIR)/setpci $(DESTDIR)$(SBINDIR)/update-pciids
+	rm -f $(DESTDIR)$(SBINDIR)/lspci $(DESTDIR)$(SBINDIR)/setpci $(DESTDIR)$(SBINDIR)/pcimodules $(DESTDIR)$(SBINDIR)/update-pciids
 	rm -f $(DESTDIR)$(IDSDIR)/$(PCI_IDS)
-	rm -f $(DESTDIR)$(MANDIR)/man8/lspci.8 $(DESTDIR)$(MANDIR)/man8/setpci.8 $(DESTDIR)$(MANDIR)/man8/update-pciids.8
+	rm -f $(DESTDIR)$(MANDIR)/man8/lspci.8 $(DESTDIR)$(MANDIR)/man8/setpci.8 $(DESTDIR)$(MANDIR)/man8/pcimodules.8 $(DESTDIR)$(MANDIR)/man8/update-pciids.8
 	rm -f $(DESTDIR)$(MANDIR)/man7/pcilib.7
 ifeq ($(SHARED),yes)
 	rm -f $(DESTDIR)$(LIBDIR)/$(PCILIB) $(DESTDIR)$(LIBDIR)/$(LIBNAME).so$(ABI_VERSION)
Index: pciutils-3.0.3/pcimodules.c
===================================================================
--- /dev/null	1970-01-01 00:00:00.000000000 +0000
+++ pciutils-3.0.3/pcimodules.c	2008-12-31 00:41:47.000000000 +0000
@@ -0,0 +1,185 @@
+/*
+ *	pcimodules:  Load all kernel modules for PCI device currently
+ *      plugged into any PCI slot.
+ *
+ *	Copyright 2000 Yggdrasil Computing, Incorporated
+ *	This file may be copied under the terms and conditions of version 
+ *      two of the GNU General Public License, as published by the Free
+ *      Software Foundation (Cambridge, Massachusetts, USA).
+ *
+ *      This file is based on pciutils/lib/example.c, which has the following
+ *      authorship and copyright statement:
+ *
+ *		Written by Martin Mares and put to public domain. You can do
+ *		with it anything you want, but I don't give you any warranty.
+ */
+
+#include <stdlib.h>
+#include <stdio.h>
+#include <malloc.h>
+#include <string.h>
+#include <unistd.h>
+#include <sys/utsname.h>
+#include <sys/param.h>
+#include <sys/types.h>
+
+#define _GNU_SOURCE
+#include <getopt.h>
+
+#include "pciutils.h"
+
+#define MODDIR	"/lib/modules"
+#define PCIMAP	"modules.pcimap"
+
+#define LINELENGTH	8000 
+
+#define DEVICE_ANY	0xffffffff
+#define VENDOR_ANY	0xffffffff
+
+#include "lib/pci.h"
+
+ const char program_name[] = "lspci";
+
+struct pcimap_entry {
+	unsigned int vendor, subsys_vendor, dev, subsys_dev, class, class_mask;
+	char *module;
+	struct pcimap_entry *next;
+};
+
+static struct pcimap_entry *pcimap_list = NULL;
+
+#define OPT_STRING "h"
+static struct option long_options[] = {
+	{"class",	required_argument,	NULL, 'c'},
+	{"classmask",	required_argument,	NULL, 'm'},
+	{"help",	no_argument,		NULL, 'h'},
+	{ 0,		0,			0, 	0}
+};
+
+static unsigned long desired_class;
+static unsigned long desired_classmask; /* Default is 0: accept all classes.*/
+
+void
+read_pcimap(void)
+{
+	struct utsname utsname;
+	char filename[MAXPATHLEN];
+	FILE *pcimap_file;
+	char line[LINELENGTH];
+	struct pcimap_entry *entry;
+	unsigned int driver_data;
+	char *prevmodule = "";
+	char module[LINELENGTH];
+
+	if (uname(&utsname) < 0) {
+		perror("uname");
+		exit(1);
+	}
+	sprintf(filename, "%s/%s/%s", MODDIR, utsname.release, PCIMAP);
+	if ((pcimap_file = fopen(filename, "r")) == NULL) {
+		perror(filename);
+		exit(1);
+	}
+
+	while(fgets(line, LINELENGTH, pcimap_file) != NULL) {
+		if (line[0] == '#')
+			continue;
+
+		entry = xmalloc(sizeof(struct pcimap_entry));
+
+		if (sscanf(line, "%s 0x%x 0x%x 0x%x 0x%x 0x%x 0x%x 0x%x",
+			   module,
+			   &entry->vendor, &entry->dev,
+			   &entry->subsys_vendor, &entry->subsys_dev,
+			   &entry->class, &entry->class_mask,
+			   &driver_data) != 8) {
+			fprintf (stderr,
+				"modules.pcimap unparsable line: %s.\n", line);
+			free(entry);
+			continue;
+		}
+
+		/* Optimize memory allocation a bit, in case someday we
+		   have Linux systems with ~100,000 modules.  It also
+		   allows us to just compare pointers to avoid trying
+		   to load a module twice. */
+		if (strcmp(module, prevmodule) != 0) {
+			prevmodule = xmalloc(strlen(module)+1);
+			strcpy(prevmodule, module);
+		}
+		entry->module = prevmodule;
+		entry->next = pcimap_list;
+		pcimap_list = entry;
+	}
+	fclose(pcimap_file);
+}
+
+/* Return a filled in pci_access->dev tree, with the device classes
+   stored in dev->aux.
+*/
+static void
+match_pci_modules(void)
+{
+	struct pci_access *pacc;
+	struct pci_dev *dev;
+	unsigned int class, subsys_dev, subsys_vendor;
+	struct pcimap_entry *map;
+	const char *prevmodule = "";
+
+	pacc = pci_alloc();		/* Get the pci_access structure */
+	/* Set all options you want -- here we stick with the defaults */
+	pci_init(pacc);		/* Initialize the PCI library */
+	pci_scan_bus(pacc);	/* We want to get the list of devices */
+  	for(dev=pacc->devices; dev; dev=dev->next) {
+		pci_fill_info(dev, PCI_FILL_IDENT | PCI_FILL_BASES);
+		class = (pci_read_word(dev, PCI_CLASS_DEVICE) << 8)
+			| pci_read_byte(dev, PCI_CLASS_PROG);
+		subsys_dev = pci_read_word(dev, PCI_SUBSYSTEM_ID);
+		subsys_vendor = pci_read_word(dev,PCI_SUBSYSTEM_VENDOR_ID);
+		for(map = pcimap_list; map != NULL; map = map->next) {
+			if (((map->class ^ class) & map->class_mask) == 0 &&
+			    ((desired_class ^ class) & desired_classmask)==0 &&
+			    (map->dev == DEVICE_ANY ||
+			     map->dev == dev->device_id) &&
+			    (map->vendor == VENDOR_ANY ||
+			     map->vendor == dev->vendor_id) &&
+			    (map->subsys_dev == DEVICE_ANY ||
+			     map->subsys_dev == subsys_dev) &&
+			    (map->subsys_vendor == VENDOR_ANY ||
+			     map->subsys_vendor == subsys_vendor) &&
+			    prevmodule != map->module) {
+				printf("%s\n", map->module);
+				prevmodule = map->module;
+			}
+		}
+
+	}
+	pci_cleanup(pacc);
+}
+
+int
+main (int argc, char **argv)
+{
+	int opt_index = 0;
+	int opt;
+
+	while ((opt = getopt_long(argc, argv, OPT_STRING, long_options,
+		           &opt_index)) != -1) {
+		switch(opt) {
+			case 'c':
+				desired_class = strtol(optarg, NULL, 0);
+				break;
+			case 'm':
+				desired_classmask = strtol(optarg, NULL, 0);
+				break;
+			case 'h':
+				printf ("Usage: pcimodules [--help]\n"
+					"  Lists kernel modules corresponding to PCI devices currently plugged"
+					"  into the computer.\n");
+		}
+	}	
+
+	read_pcimap();
+	match_pci_modules();
+	return 0;
+}
Index: pciutils-3.0.3/pcimodules.man
===================================================================
--- /dev/null	1970-01-01 00:00:00.000000000 +0000
+++ pciutils-3.0.3/pcimodules.man	2008-12-31 00:41:47.000000000 +0000
@@ -0,0 +1,92 @@
+.TH pcimodules 8 "@TODAY@" "@VERSION@" "Linux PCI Utilities"
+.IX pcimodules
+.SH NAME
+pcimodules \- List kernel driver modules available for all currently plugged
+in PCI devices
+.SH SYNOPSIS
+.B pcimodules
+.RB [ --class class_id ]
+.RB [ --classmask mask ]
+.RB [ --help ]
+.SH DESCRIPTION
+.B pcimodules
+lists all driver modules for all currently plugged in PCI devices.
+.B pcimodules
+should be run at boot time, and whenever a PCI device is "hot plugged"
+into the system.  This can be done by the following Bourne shell syntax:
+.IP
+	for module in $(pcimodules) ; do
+.IP
+		modprobe -s -k "$module"
+.IP
+	done
+.PP
+When a PCI device is removed from the system, the Linux kernel will
+decrement a usage count on PCI driver module.  If this count drops
+to zero (i.e., there are no PCI drivers), then the
+.B modprobe -r
+process that is normally configured to run from cron every few minutes
+will eventually remove the unneeded module.
+.PP
+The --class and --classmask arguments can be used to limit the search
+to certain classes of PCI devices.  This is useful, for example, to
+generate a list of ethernet card drivers to be loaded when the kernel
+has indicated that it is trying to resolve an unknown network interface.
+.PP
+Modules are listed in the order in which the PCI devices are physically
+arranged so that the computer owner can arrange things like having scsi
+device 0 be on a controller that is not alphabetically the first scsi
+controller.
+.SH OPTIONS
+.TP
+.B --class class --classmask mask
+.PP
+--class and --classmask limit the search to PCI
+cards in particular classes.  These arguments are always used together.
+The arguments to --class and --classmask
+can be given as hexadecimal numbers by prefixing a leading "0x".
+Note that the classes used by pcimodules are in "Linux" format,
+meaning the class value that you see with lspci would be shifted
+left eight bits, with the new low eight bits programming interface ID.
+An examples of how to use class and classmask is provided below.
+.B --help, -h
+Print a help message and exit.
+.SH EXAMPLES
+.TP
+pcimodules
+lists all modules corresponding to currently plugged in PCI devices.
+.TP
+pcimodules --class 0x200000 --classmask 0xffff00
+lists all modules corresponding to currently plugged in ethernet PCI devices.
+.SH FILES
+.TP
+.B /lib/modules/<kernel-version>/modules.pcimap
+This file is automatically generated by
+.B depmod,
+and used by
+.B pcimodules
+to determine which modules correspond to which PCI ID's.
+.TP
+.B /proc/bus/pci
+An interface to PCI bus configuration space provided by the post-2.1.82 Linux
+kernels. Contains per-bus subdirectories with per-card config space files and a
+.I devices
+file containing a list of all PCI devices.
+
+.SH SEE ALSO
+.BR lspci (8)
+
+.SH MAINTAINER
+The Linux PCI Utilities are maintained by Martin Mares <mj@suse.cz>.
+
+.SH AUTHOR
+.B pcimodules
+was written by Adam J. Richter <adam@yggdrasil.com>, based on public
+domain example code by Martin Mares <mj@suse.cz>.
+
+.SH COPYRIGHT
+.B pcimodules
+is copyright 2000, Yggdrasil Computing, Incorporated, and may
+be copied under the terms and conditions of version 2 of the GNU
+General Public License as published by the Free Software Foundation
+(Cambrige, Massachusetts, United States of America).
